    SiS IDE Driver Installation For OS/2
    ====================================

[Install from Floppy]
===============================================
1. Open OS2 Windows or OS2 Full Screen.
2. Change Directory to A:\OS2.
3. Run INSTOS2.EXE
4. Reboot OS/2 system.
===============================================

[Install from CD-ROM]
===============================================
1. Put the Driver CD in CD-ROM Drive.
2. Open OS2 Windows or OS2 Full Screen.
3. Change Drive to CD-ROM Drive.
4. Change Directory to \IDE\OS2.
5. Run INSTOS2.EXE
6. Reboot OS/2 system.
===============================================

[Note 1] Default Transfer Mode is ^Master DMA Mode
[Note 2] Add /!M option after BASEDEV=SISIDE.ADD in
         CONFIG.SYS to disable ^Master DMA Mode
